**Maximum loads of grab rails, CARE-products and additional loads of towel rails – TÜV certificated**

**Grab rails in general max. 160 kg**

***TÜV certificate!***

**Towel rails in general max. 25 kg**

***Only in-house testing!* The load is set up in centre of the towel rail tubes**

**Tip-up seat 01680 max. 125 kg**

***TÜV certificate!***

**Tip-up seat 14980 fixed max. 130 kg**

***TÜV certificate!***

**Bathroom stool 14982 / 11682 max. 100 kg**

***TÜV certificate!***

**Tip-up seat 14983 wall mounted max. 150kg**

***TÜV certificate!***

**Plan Care products**

**Grab rail 34901 up to 1100 mm max. 130 kg**

***TÜV certificate!***

**Pivoted supporting rails 34902/03/04/05 max. 100 kg**

***TÜV certificate!* The load is set up at the front cover**

**Angle bars 34906/07/08/11/12/14/15 max. 130 kg**

***TÜV certificate!***

**Tip-up seats 34980/81/82 max. 130 kg**

***TÜV certificate!* The load is set up in centre of the seat**

**Tip-up seat 34981 max. 130 kg**

**for rail system/hinged**

***TÜV certificate!***

**Tip-up seat 34982 max. 130 kg**

**with fixed back rest**

***TÜV certificate!***

**Tip-up seat 34983 wall mounted max. 150 kg**

***TÜV certificate!***