**Maximum load capacity of AXESS Products TÜV certificated.**

**Bathroom stool** 35082010037 – load capacity 150kg

**AXESS Grab Bars** 35001XXXXXX– load capacity 115kg.

**Drop Down Supporting Rail** 35003xxxxxx **–** load capacity 115kg.

**Angle bar 90°** 35006XX0801 and 35006XX0802 – load capacity 115kg

**Rail system** 35008XX6601, 35014XX7013, 35015XX0101, 35015XX0102, and 35008XX6602 – load capacity 115kg

**Angle bar 90° Hand shower sliding rail -** 35006XX1301 and

35006XX1302 load capacity 115kg

**Hand shower sliding rail** 35012XX0800 load capacity 115kg.

**Corner rail for Shower/Bath** 35011XX6801 load capacity 115kg